IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2022-06-19T01:51:33"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210420_1515(x64) - Exporter 20.2.40.65 - Alternate UI 20.2.40.65"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "Dhiagan-Chetty" of Organization (no name given)
  Owner history of Person "Dhiagan-Chetty" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1655230058 (2022-06-14T18:07:38Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Base Level" | long name "Base Level" | object type "Level:Level 1" | elevation 0.
        contains 3 elements
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:PW06 - JUMBO MoistureWALL 63/30" | object type "Curtain Wall:PW06 - JUMBO MoistureWALL 63/30" | names: "Curtain Wall:PW06 - JUMBO MoistureWALL 63/30:4178" | parts: 76 IFCMEMBER, 25 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:4561" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:PW06 - JUMBO MoistureWALL 63/30" | object type "Basic Wall:PW06 - JUMBO MoistureWALL 63/30" | names: "Basic Wall:PW06 - JUMBO MoistureWALL 63/30:5314" | material: layers "Basic Wall:PW06 - JUMBO MoistureWALL 63/30" ("Gypsum Wall Board" 12., "Metal Stud Layer" 65., "Gypsum Wall Board" 12.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Types
  IFCCURTAINWALLTYPE "Curtain Wall:PW06 - JUMBO MoistureWALL 63/30" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:PW06 - JUMBO MoistureWALL 63/30" | STANDARD | 1 occurrence | material: layers "Basic Wall:PW06 - JUMBO MoistureWALL 63/30" ("Gypsum Wall Board" 12., "Metal Stud Layer" 65., "Gypsum Wall Board" 12.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Property sets
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "PW06 - JUMBO MoistureWALL 63/30" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "PW06 - JUMBO MoistureWALL 63/30" (IFCIDENTIFIER)
  Pset_ProductRequirements | properties | on 76 objects (76 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
  Pset_ProductRequirements | properties | on 25 objects (25 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCWALLSTANDARDCASE) | on 2 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Base Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 76 objects (76 IFCMEMBER)
    Reference = "Stud Mullion - 63mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 25 objects (25 IFCPLATE)
    Reference = "2 Layer - 12mm Drywall Panels 89mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCWALLSTANDARDCASE) | on 2 type objects
    Reference = "PW06 - JUMBO MoistureWALL 63/30" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 25 objects (25 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2 Layer - 12mm Drywall Panels 89mm" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 48 objects (48 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Stud Mullion - 63mm" (IFCIDENTIFIER)
    Span = 581.000000304797 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 26 objects (26 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Stud Mullion - 63mm" (IFCIDENTIFIER)
    Span = 3000.00000000014 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Stud Mullion - 63mm" (IFCIDENTIFIER)
    Span = 161.999999695203 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "PW06 - JUMBO MoistureWALL 63/30" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "PW06 - JUMBO MoistureWALL 63/30" (IFCIDENTIFIER)
    ThermalTransmittance = 0.384615384615385 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "PW06 - JUMBO MoistureWALL 63/30" (IFCIDENTIFIER)
    ThermalTransmittance = 0.384615384615385 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Base Level" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)

Other addresses and roles
  2 x postal address (none given)