IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2022-06-14T21:46:11"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210420_1515(x64) - Exporter 20.2.40.65 - Alternate UI 20.2.40.65"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "Dhiagan-Chetty" of Organization (no name given)
  Owner history of Person "Dhiagan-Chetty" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1655233917 (2022-06-14T19:11:57Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Base Level" | long name "Base Level" | object type "Level:Level 1" | elevation 0.
        contains 18 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):2477" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Bottom Hung" | object type "Ceiling_Access_HatchPanel_Parametric:Bottom Hung" | names: "Ceiling_Access_HatchPanel_Parametric:Bottom Hung:2482" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | object type "Basic Wall:190mm MAXI BLOCK- plastered" | names: "Basic Wall:190mm MAXI BLOCK- plastered:2488" | material: "_np_Brickwork - Plastered" | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:2491" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCDOOR | type IFCDOORSTYLE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:2496", "M_Single-Flush:0915 x 2134mm:2524" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | object type "Basic Wall:190mm MAXI BLOCK- plastered" | names: "Basic Wall:190mm MAXI BLOCK- plastered:2497", "Basic Wall:190mm MAXI BLOCK- plastered:2523", "Basic Wall:190mm MAXI BLOCK- plastered:2525" | material: layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Shadowline used with econogrid" | object type "TR01:Pelican Systems Shadowline used with econogrid" | names: "TR01:Pelican Systems Shadowline used with econogrid:2499" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Shadowline used with econogrid" | object type "TR01:Pelican Systems Shadowline used with econogrid" | names: "TR01:Pelican Systems Shadowline used with econogrid:2501" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          4 x IFCWINDOW | type IFCWINDOWSTYLE "0610 x 0610mm" | object type "M_Fixed:0610 x 0610mm" | names: "M_Fixed:0610 x 0610mm:2514", "M_Fixed:0610 x 0610mm:2515", "M_Fixed:0610 x 0610mm:2528" (+1 more) | material: materials ("Glass", "Sash") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:AMF Thermatex® Star - 600x600mm" | object type "Compound Ceiling:AMF Thermatex® Star - 600x600mm" | CEILING | names: "Compound Ceiling:AMF Thermatex® Star - 600x600mm:2518" | material: layers "Compound Ceiling:AMF Thermatex® Star - 600x600mm" ("Ceiling Tile - Smooth Tile with Perforations 600 x 600(1)" 36., "Ceiling Tile - Smooth Tile with Perforations 600 x 600" 15.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Shadowline used with econogrid" | object type "TR01:Pelican Systems Shadowline used with econogrid" | names: "TR01:Pelican Systems Shadowline used with econogrid:2527" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" | object type "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" | CEILING | names: "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2:2558" | material: layers "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" ("Ceiling Tile - Smooth Tile with Perforations 600 x 600" 1., "Ceiling Tile - Smooth Tile with Perforations 600 x 600" 15.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Bottom Hung" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | STANDARD | 4 occurrences | material: layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "0915 x 2134mm" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:2496
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Shadowline used with econogrid" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Shadowline used with econogrid" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWINDOWSTYLE "0610 x 0610mm" | 4 occurrences | material: materials ("Glass", "Sash") | property sets: M_Fixed:0610 x 0610mm:2514
  IFCCOVERINGTYPE "Compound Ceiling:AMF Thermatex® Star - 600x600mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Shadowline used with econogrid" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" (IFCIDENTIFIER)
    TotalThickness = 11. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Ceiling Tile - Smooth Tile with Perforations 600 x 600;" (IFCTEXT)
    Reference = "AMF Thermatex® Star - 600x600mm" (IFCIDENTIFIER)
    TotalThickness = 51. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Ceiling Tile - Smooth Tile with Perforations 600 x 600;" (IFCTEXT)
    Reference = "AMF Thermatex® Star - 600x600mm 2" (IFCIDENTIFIER)
    TotalThickness = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    Reference = "AMF Thermatex® Star - 600x600mm" (IFCIDENTIFIER)
    TotalThickness = 51. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    Reference = "AMF Thermatex® Star - 600x600mm 2" (IFCIDENTIFIER)
    TotalThickness = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ElementShading | properties | on 8 objects (3 IFCCOVERING, 3 IFCWALLSTANDARDCASE, 1 IFCSLAB, 1 IFCWALL) | on 5 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 4 objects (4 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 3 objects (3 IFCCOVERING) | on 3 type objects
    Category = "Ceilings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCDOOR)
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Base Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 4 objects (4 IFCWINDOW)
    Reference = "0610 x 0610mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "Pelican Systems Shadowline used with econogrid" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCDOOR)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Bottom Hung" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Generic Floor - 250mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "AMF Thermatex® Star - 600x600mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 1 more content on 1 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "Pelican Systems Shadowline used with econogrid" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Bottom Hung" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL) | on 1 type object
    Reference = "190mm MAXI BLOCK- plastered" (IFCLABEL)
  Pset_WallCommon | properties | on 4 objects (3 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Generic Floor - 250mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic Floor - 250mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Floor - 250mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0610 x 0610mm" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    Manufacturer = "AMF (through Pelican Systems)" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Base Level" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  M_Single-Flush:0915 x 2134mm:2496 | predefined | on 2 type objects
  M_Fixed:0610 x 0610mm:2514 | predefined | on 1 type object

Other addresses and roles
  2 x postal address (none given)