IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2022-06-14T22:42:28"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210420_1515(x64) - Exporter 20.2.40.65 - Alternate UI 20.2.40.65"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "Dhiagan-Chetty" of Organization (no name given)
  Owner history of Person "Dhiagan-Chetty" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1655235697 (2022-06-14T19:41:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Base Level" | long name "Base Level" | object type "Level:Level 1" | elevation 0.
        contains 10 elements
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | object type "Basic Wall:190mm MAXI BLOCK- plastered" | names: "Basic Wall:190mm MAXI BLOCK- plastered:2480", "Basic Wall:190mm MAXI BLOCK- plastered:2489" | material: layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCDOOR | type IFCDOORSTYLE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:2481", "M_Single-Flush:0915 x 2134mm:2490" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" | object type "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" | CEILING | names: "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2:2484" | material: layers "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" ("Ceiling Tile - Smooth Tile with Perforations 600 x 600" 1., "Ceiling Tile - Smooth Tile with Perforations 600 x 600" 15.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Plaster Ceiling Junction" | object type "TR14:Trims Plaster Ceiling Junction" | names: "TR14:Trims Plaster Ceiling Junction:2492" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Plaster Ceiling Junction" | object type "TR14:Trims Plaster Ceiling Junction" | names: "TR14:Trims Plaster Ceiling Junction:2494" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm:2521" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm" ("ceiling Flush Plastered - 12mm" 9.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Flushline Outer Frame" | object type "Flushline Outer Frame:Flushline Outer Frame" | names: "Flushline Outer Frame:Flushline Outer Frame:2526" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):2529" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | STANDARD | 2 occurrences | material: layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCDOORSTYLE "0915 x 2134mm" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:2481
  IFCCOVERINGTYPE "Compound Ceiling:AMF Thermatex® Star - 600x600mm 2" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Plaster Ceiling Junction" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Plaster Ceiling Junction" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Flushline Outer Frame" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Pset_ElementShading | properties | on 5 objects (3 IFCCOVERING, 2 IFCWALLSTANDARDCASE) | on 4 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 3 objects (3 IFCCOVERING) | on 3 type objects
    Category = "Ceilings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCDOOR)
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Base Level" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Trims Plaster Ceiling Junction" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCDOOR)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "AMF Thermatex® Star - 600x600mm 2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Flushline Outer Frame" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "190mm MAXI BLOCK- plastered" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT) - 9 mm" (IFCIDENTIFIER)
    TotalThickness = 9. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" (IFCIDENTIFIER)
    TotalThickness = 11. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Ceiling Tile - Smooth Tile with Perforations 600 x 600;" (IFCTEXT)
    Reference = "AMF Thermatex® Star - 600x600mm 2" (IFCIDENTIFIER)
    TotalThickness = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    Reference = "AMF Thermatex® Star - 600x600mm 2" (IFCIDENTIFIER)
    TotalThickness = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Manufacturer = "AMF (through Pelican Systems)" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Trims Plaster Ceiling Junction" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Flushline Outer Frame" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Base Level" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  M_Single-Flush:0915 x 2134mm:2481 | predefined | on 2 type objects

Other addresses and roles
  2 x postal address (none given)