IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2022-10-21T22:39:10"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20220517_1515(x64) - Exporter 20.2.90.12 - Default UI"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "dhiaganKBRNF" of Organization (no name given)
  Owner history of Person "dhiaganKBRNF" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1666371442 (2022-10-21T16:57:22Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "GROUND FLOOR" | long name "GROUND FLOOR" | object type "Level:Level 1" | elevation 0.
        contains 133 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):389079" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "In Lay" | object type "Ceiling_Access_HatchPanel_Parametric:In Lay" | names: "Ceiling_Access_HatchPanel_Parametric:In Lay:389084" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          9 x IFCWALL | type IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | object type "Basic Wall:190mm MAXI BLOCK- plastered" | names: "Basic Wall:190mm MAXI BLOCK- plastered:389085", "Basic Wall:190mm MAXI BLOCK- plastered:389143", "Basic Wall:190mm MAXI BLOCK- plastered:389206" (+6 more) | material: "_np_Brickwork - Plastered"; layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:389088" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          9 x IFCDOOR | type IFCDOORSTYLE "0915 x 2134mm" | object type "M_Single-Flush:0915 x 2134mm" | names: "M_Single-Flush:0915 x 2134mm:389093", "M_Single-Flush:0915 x 2134mm:389151", "M_Single-Flush:0915 x 2134mm:389214" (+6 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | object type "Basic Wall:190mm MAXI BLOCK- plastered" | names: "Basic Wall:190mm MAXI BLOCK- plastered:389094", "Basic Wall:190mm MAXI BLOCK- plastered:389152", "Basic Wall:190mm MAXI BLOCK- plastered:389215" (+6 more) | material: layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "office_workstation_14935" | object type "office_workstation_14935:office_workstation_14935" | names: "office_workstation_14935:office_workstation_14935:389095", "office_workstation_14935:office_workstation_14935:389153", "office_workstation_14935:office_workstation_14935:389216" (+6 more) | material: materials ("Mac-Screen Inner", "Mac-Screen", "Mac-Body", "Default Wall", "Steel, Wrought", "Polypropylene", "Plastic, Opaque White") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Chair-Task Arms" | object type "Chair-Task Arms:Chair-Task Arms" | names: "Chair-Task Arms:Chair-Task Arms:389096", "Chair-Task Arms:Chair-Task Arms:389154", "Chair-Task Arms:Chair-Task Arms:389217" (+6 more) | material: materials ("Textile - Slate Blue", "Plastic - Black") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:389098" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:389100" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:389102" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          18 x IFCWINDOW | type IFCWINDOWSTYLE "0610 x 0610mm" | object type "M_Fixed:0610 x 0610mm" | names: "M_Fixed:0610 x 0610mm:389103", "M_Fixed:0610 x 0610mm:389104", "M_Fixed:0610 x 0610mm:389161" (+15 more) | material: materials ("Glass", "Sash") | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):389137" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Flushline Outer Frame" | object type "Flushline Outer Frame:Flushline Outer Frame" | names: "Flushline Outer Frame:Flushline Outer Frame:389142" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:389146" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:389156" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:389158" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:389160" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):389200" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "In Lay" | object type "Ceiling_Access_HatchPanel_Parametric:In Lay" | names: "Ceiling_Access_HatchPanel_Parametric:In Lay:389205" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:389209" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:389219" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:389221" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:389223" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          11 x IFCBUILDINGELEMENTPROXY | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:389535", "Model Text:600mm Arial:389537", "Model Text:600mm Arial:389538" (+8 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):496639" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "In Lay" | object type "Ceiling_Access_HatchPanel_Parametric:In Lay" | names: "Ceiling_Access_HatchPanel_Parametric:In Lay:496644" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:496648" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:496658" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:496660" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:496662" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):496667" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Top Hung" | object type "Ceiling_Access_HatchPanel_Parametric:Top Hung" | names: "Ceiling_Access_HatchPanel_Parametric:Top Hung:496672" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:496676" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:496686" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:496690" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):496695" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Flushline Outer Frame" | object type "Flushline Outer Frame:Flushline Outer Frame" | names: "Flushline Outer Frame:Flushline Outer Frame:496700" | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:496704" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:496714" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:496716" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:496718" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):496749" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:496758" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):496777" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:496786" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | object type "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | names: "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT):496805" | material: layers "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" ("ceiling Flush Plastered - 12mm" 11.) | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 250mm" | object type "Floor:Generic Floor - 250mm" | FLOOR | names: "Floor:Generic Floor - 250mm:496814" | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "PS2 Corner Trim - Internal:Pelican Systems Plaster Trim 25 x 20" | names: "PS2 Corner Trim - Internal:Pelican Systems Plaster Trim 25 x 20:509187" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 35 x 35" | object type "PS3 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 35 x 35" | names: "PS3 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 35 x 35:509655", "PS3 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 35 x 35:558501" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "PS4 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 45 x 20" | names: "PS4 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 45 x 20:509664" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:510597" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "TR02:Pelican Systems Plaster Trim 25 x 20" | names: "TR02:Pelican Systems Plaster Trim 25 x 20:510609" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "PS2 Corner Trim - External:Pelican Systems Plaster Trim 25 x 20" | names: "PS2 Corner Trim - External:Pelican Systems Plaster Trim 25 x 20:510704", "PS2 Corner Trim - External:Pelican Systems Plaster Trim 25 x 20:558503" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:511076" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "TR04:Trims Pelican Systems Plaster Trim 45 x 20" | names: "TR04:Trims Pelican Systems Plaster Trim 45 x 20:511104" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 35 x 35" | object type "PS3 Corner Trim - External:Trims Pelican Systems Plaster Trim 35 x 35" | names: "PS3 Corner Trim - External:Trims Pelican Systems Plaster Trim 35 x 35:511164" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:511426" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | object type "TR05:Trims Pelican Systems Plaster Trim 45 x 45" | names: "TR05:Trims Pelican Systems Plaster Trim 45 x 45:511467" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "PS4 Corner Trim - External:Trims Pelican Systems Plaster Trim 45 x 20" | names: "PS4 Corner Trim - External:Trims Pelican Systems Plaster Trim 45 x 20:511533" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | object type "Corner Trim - Internal - Demo:Pelican Systems Plaster Trim 25 x 20" | names: "Corner Trim - Internal - Demo:Pelican Systems Plaster Trim 25 x 20:558500" | material: materials ("__Metal-Steel", "Shim", "FABER WATER GLASS") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "PS4 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 45 x 20" | names: "PS4 Corner Trim - Internal:Trims Pelican Systems Plaster Trim 45 x 20:558502" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 35 x 35" | object type "PS3 Corner Trim - External:Trims Pelican Systems Plaster Trim 35 x 35" | names: "PS3 Corner Trim - External:Trims Pelican Systems Plaster Trim 35 x 35:558504" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | object type "PS4 Corner Trim - External:Trims Pelican Systems Plaster Trim 45 x 20" | names: "PS4 Corner Trim - External:Trims Pelican Systems Plaster Trim 45 x 20:558505" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "In Lay" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Basic Wall:190mm MAXI BLOCK- plastered" | STANDARD | 18 occurrences | material: layers "Basic Wall:190mm MAXI BLOCK- plastered" ("_np_Brickwork - Plastered" 190.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCDOORSTYLE "0915 x 2134mm" | SINGLE_SWING_RIGHT | 9 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2134mm:389093
  IFCFURNITURETYPE "office_workstation_14935" | 9 occurrences | material: materials ("Mac-Screen Inner", "Mac-Screen", "Mac-Body", "Default Wall", "Steel, Wrought", "Polypropylene", "Plastic, Opaque White")
  IFCFURNITURETYPE "Chair-Task Arms" | 9 occurrences | material: materials ("Textile - Slate Blue", "Plastic - Black")
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWINDOWSTYLE "0610 x 0610mm" | 18 occurrences | material: materials ("Glass", "Sash") | property sets: M_Fixed:0610 x 0610mm:389103
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Flushline Outer Frame" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "In Lay" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "In Lay" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Top Hung" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Flushline Outer Frame" | 1 occurrence | material: "mesh" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCCOVERINGTYPE "Compound Ceiling:_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" | CEILING | 1 occurrence | property sets: Pset_CoveringCommon, Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCSLABTYPE "Floor:Generic Floor - 250mm" | FLOOR | 1 occurrence | material: layers "Floor:Generic Floor - 250mm" ("_Generic Model White" 250.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 35 x 35" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 35 x 35" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 45" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Pelican Systems Plaster Trim 25 x 20" | 1 occurrence | material: materials ("__Metal-Steel", "Shim", "FABER WATER GLASS") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 35 x 35" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Trims Pelican Systems Plaster Trim 45 x 20" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Pset_CoveringCommon | properties | on 9 objects (9 IFCCOVERING) | on 9 type objects
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" (IFCIDENTIFIER)
    TotalThickness = 11. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ElementShading | properties | on 36 objects (9 IFCCOVERING, 9 IFCSLAB, 9 IFCWALL, 9 IFCWALLSTANDARDCASE) | on 19 type objects
    Roughness = 304.8 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_ProductRequirements | properties | on 52 objects (52 IFCBUILDINGELEMENTPROXY) | on 39 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 18 objects (9 IFCWALL, 9 IFCWALLSTANDARDCASE) | on 1 type object
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 18 objects (18 IFCFURNISHINGELEMENT)
    Category = "Furniture" (IFCLABEL)
  Pset_ProductRequirements | properties | on 18 objects (18 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
  Pset_ProductRequirements | properties | on 9 objects (9 IFCCOVERING) | on 9 type objects
    Category = "Ceilings" (IFCLABEL)
  Pset_ProductRequirements | properties | on 9 objects (9 IFCSLAB) | on 9 type objects
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 9 objects (9 IFCDOOR)
    Category = "Doors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "GROUND FLOOR" (IFCLABEL)
  Pset_ProductRequirements: 1 more content on 1 objects not shown
  Pset_QuantityTakeOff | properties | on 18 objects (9 IFCWALL, 9 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 18 objects (18 IFCWINDOW)
    Reference = "0610 x 0610mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 12 type objects
    Reference = "Trims Pelican Systems Plaster Trim 45 x 20" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 11 type objects
    Reference = "Pelican Systems Plaster Trim 25 x 20" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (9 IFCCOVERING) | on 9 type objects
    Reference = "_C2.3 - 12mm FLUSHPLASTER CEILING (UNDER CONCRETE SOFFIT)" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (9 IFCSLAB) | on 9 type objects
    Reference = "Generic Floor - 250mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 9 objects (9 IFCDOOR)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 7 more contents on 35 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 12 type objects
    Reference = "Trims Pelican Systems Plaster Trim 45 x 20" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 11 type objects
    Reference = "Pelican Systems Plaster Trim 25 x 20" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 11 objects (11 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY) | on 7 type objects
    Reference = "Trims Pelican Systems Plaster Trim 45 x 45" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "Trims Pelican Systems Plaster Trim 35 x 35" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "In Lay" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Flushline Outer Frame" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Top Hung" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfWall | properties | on 18 objects (9 IFCWALL, 9 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "190mm MAXI BLOCK- plastered" (IFCLABEL)
  Pset_WallCommon | properties | on 18 objects (9 IFCWALL, 9 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "190mm MAXI BLOCK- plastered" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfSlab | properties | on 9 objects (9 IFCSLAB) | on 9 type objects
    Reference = "Generic Floor - 250mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 9 objects (9 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic Floor - 250mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 9 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Floor - 250mm" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "0915 x 2134mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 18 objects (18 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0610 x 0610mm" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "GROUND FLOOR" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  M_Single-Flush:0915 x 2134mm:389093 | predefined | on 2 type objects
  M_Fixed:0610 x 0610mm:389103 | predefined | on 1 type object

Other addresses and roles
  2 x postal address: "## Street City, State Zip", "Boston", "MA"